**UDP4303S DC Power Supply Firmware Upgrade Guide**

* **Prepare the Upgrade File**

Select the appropriate upgrade file according to your instrument model and copy it to the root directory of a USB flash drive formatted in FAT32.

* **Check the Current Version**

Press the MENU button, navigate to the Setup interface, and select About to view the current firmware version. Ensure that the new version is higher than the existing one.

图形用户界面

AI 生成的内容可能不正确。图片包含 图形用户界面

AI 生成的内容可能不正确。

* **Insert USB Flash Drive**

Insert the prepared USB drive into the device’s USB port. A notification will appear once the USB drive is recognized.

* **Select Upgrade File**

Go to Upgrade > File, browse the D drive, locate the upgrade file, and click Select to confirm.

图片包含 日程表

AI 生成的内容可能不正确。

* **Verify Version Information**

The system will display both the current and target firmware versions. After verifying the information, click Start.

* **Start Upgrade Process**

In the pop-up confirmation window, select **Yes** to begin the upgrade process.

图片包含 文本




AI 生成的内容可能不正确。图片包含 图形用户界面

AI 生成的内容可能不正确。

* **Wait for Completion**

The upgrade process will go through several stages such as **Checking**, **Programming**, and **Updating**.


⚠️ Do not power off the device during the upgrade.



* **Finish the Upgrade**

Once the message “Successfully! Please reboot the device." appears, the upgrade is complete.

Restart the instrument as instructed.



* **Verify Upgrade**

After restarting, go to Setup > About again to confirm the firmware version has been updated successfully.

图片包含 图形用户界面

AI 生成的内容可能不正确。