# Upgrade Guide


**Upgrade through the system interface**

1、Check the current hardware version of the UTG2000A. Download the appropriate version of firmware from the official website.


Utility->System->About




2、Save the firmware for upgrading in the root directory of the U drive.



3、Insert the USB disk into the USB port of UTG2000A. The instrument will recognize the U drive, press Utility->System->Software Upgrading in order, select the upgrade file of the corresponding model through the knob and confirm.



4、Wait for the upgrade to complete and the instrument will restart automatically without intervention.



5、After the instrument reboots, unplug the USB flash drive. Enter the System Information page to view the current version information.

