
# Upgrade Guide


**Upgrade via software on the host computer（Device Manager）**

1、Since the UTG900E series does not have a USB HOST interface, the firmware will be upgraded through the host computer software. Check the current hardware version of UTG900E. Check the current hardware version of UTG900E and download the corresponding version or higher firmware from the official website.


Utility->System->->Page Down->About




2、Save the firmware to your computer disk.




3、Install and start the host computer software, right-click on the UTG900E device that appears, and select "Open AWG" to open the virtual control panel of the device.



4、In the virtual panel, in the device display area, right mouse button select “Send Firmware Program”



5、In the pop-up dialog box, ""Firmware Program"" is for device firmware upgrade, and "FPGA Firmware Program" is for device logic upgrade. Click "..." on the right to select the corresponding file.



6、After selecting the firmware, click "Update" to start upgrading, the device will automatically reboot during the upgrade process, until the bottom right corner appears "Program upgrade successfully", that is, the upgrade is complete!

